{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["ACB Selections","ACB Schedule","Throw Data","Statistics","Backend Data","ACB Format Handler","Data Validation","Username Archive","Changelog"],"not_rendered":{"charts":0,"images":33,"macros":1,"external_links":0,"defined_names":19,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ACB Selections","index":0,"n_rows":21,"n_cols":56,"rows_kept":21,"cut":false,"hidden":false,"merged":[[16,31,16,32],[16,33,16,34],[14,1,14,2],[14,3,14,6],[16,12,16,25],[16,28,16,29],[10,1,10,2],[11,1,11,2],[13,1,13,2],[12,1,12,2],[12,3,12,6],[13,3,13,6],[10,3,10,6],[11,3,11,6],[18,9,18,11],[16,9,16,11],[16,1,18,1],[16,2,18,2],[18,4,18,6],[16,4,16,8],[16,3,17,3],[17,8,18,8],[10,8,12,8],[6,17,6,18],[18,50,18,55],[17,12,18,12],[17,13,18,13],[18,38,18,42],[18,45,18,47],[18,43,18,44],[18,48,18,49],[17,24,18,24],[17,18,18,18],[6,22,6,23],[5,14,6,14],[5,20,6,20],[10,14,11,14],[16,26,16,27],[18,35,18,36],[0,1,3,25],[16,50,16,55],[16,45,16,49],[16,37,16,44],[5,8,6,8],[14,26,14,36],[15,26,15,30],[15,31,15,34],[15,35,15,36],[12,11,12,12],[10,9,11,9],[10,10,11,10],[10,11,11,11],[10,12,11,12],[10,13,11,13]]}
[1]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Room Conditions","Dry Bulb","Relative Humidity","Dew Point","On-Coil Air Temp",null,"Primary Air Conditions","Dry Bulb","Relative Humidity","Wet Bulb","Dew Point",null,"Entering Water Conditions","Entering Water","Propylene Glycol","Ethylene Gylcol",null,"Elevation"]
[null,null,null,null,null,null,null,null,null,"°F","%","°F","°F",null,null,"°F","%","°F",null,null,null,"°F","%",null,null,"ft"]
[null,null,null,null,null,null,null,null,"Cooling",75,50,55.1,75,null,"Cooling",55,78,51.3,48.3,null,"Cooling",57,0,0,null,0]
[null,null,null,null,null,null,null,null,"Heating",70,50,50.5,null,null,"Heating",55,50,46,36.799999999999997,null,"Heating",120,0,0]
[]
[null,"Project Name:",null,null,null,null,null,null,"Selection Criteria","Air ∆P","Water ∆P","Water Flow\n(Cooling)","Water Flow\n(Heating)","Sound Level","Primary Air / Unit Length"]
[null,"Project Number:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Software Designed and Coded by Christopher Oski"]
[null,"Version:",null,null,null,null,null,null,null,"Inch WC","ft WC","GPM",null,"NC","CFM / Lft"]
[null,"Date:",null,"2019-04-03",null,null,null,null,"Min",0.2,0.1,0.5,0.2,0,3]
[null,"Software Version:",null,1,null,null,null,null,"Max",0.7,11,2.4,2.4,35,20,null,null,null,null,null,null,null,null,null,null,null,"Local Design Conditions"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Room Conditions",null,null,null,null,"Primary Air Conditions",null,null,null,"Entering Water"]
[null,"Unit Tag","Zone Name or Number","Area","Design Requirements Per Zone",null,null,null,null,"Total Load Difference",null,null,"Design Criteria Per Unit",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling",null,"Heating",null,"Cooling","Cooling",null,"Heating",null,"Cooling","Heating","Cooling Data Per Unit",null,null,null,null,null,null,null,"Heating Data Per Unit",null,null,null,null,"Sound Power Levels (No Attenuation)"]
[null,null,null,null,"Sensible Load","Latent Load","Heating Load","Minimum Primary Airflow","Number of Units","Sensible","Latent","Heating","Model","2 or 4 Pipe\n\n","Model Length","Target Primary Air Pressure","Actual Pressure","Primary Airflow Rate","Nozzle Config.\n\n","Chilled Water Flow Rate","Water Pressure Drop (Cooling)","Heating Water Flow Rate","Water Pressure Drop (Heating)","Primary Air Inlet Size","Spigot Shape","Sound Level\nWith\n3 dB Atten.","Dry Bulb","Relative Humidity","Dry Bulb","Relative Humidity","On-Coil Air Temp","Dry Bulb","Relative Humidity","Dry Bulb","Relative Humidity","Entering Water","Entering Water","Supply Airflow Rate","Primary Air Sensible","Primary Air Latent","Secondary Air Sensible","Net Unit Sensible","Total Capacity","Leaving Water Temp","Supply Air Temp Out","Primary Air Offset Capacity","Coil Capacity","Net Unit Capacity","Leaving Water Temp","Supply Air Temp Out","125 Hz","250 Hz","500 Hz","1000 Hz","2000 Hz","4000 Hz"]
[null,null,null,"ft2","BTUH",null,null,"CFM",null,"BTUH",null,null,null,null,"ft","Inch WC","Inch WC","CFM",null,"GPM","ft WC","GPM","ft WC","Inch",null,"NC","°F","%","°F","%","°F","°F","%","°F","%","°F",null,"CFM","BTUH",null,null,null,null,"°F",null,"BTUH",null,null,"°F",null,"dB"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB40",null,2,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Unit"]

{"sheet":"ACB Schedule","index":1,"n_rows":21,"n_cols":51,"rows_kept":21,"cut":false,"hidden":true,"merged":[[16,47,16,49],[8,21,8,22],[5,21,5,26],[0,1,3,29],[6,21,6,22],[6,24,6,25],[7,21,7,22],[7,24,7,25],[6,17,6,18],[7,17,7,18],[5,11,5,19],[6,11,6,12],[7,11,7,12],[8,11,8,12],[6,14,6,15],[7,14,7,15],[8,14,8,15],[6,7,6,8],[7,7,7,8],[8,7,8,8],[5,7,5,9],[18,47,18,48],[10,22,11,22],[10,24,11,24],[10,19,12,19],[10,16,11,16],[10,17,11,17],[10,20,11,20],[10,21,11,21],[16,41,16,46],[18,41,18,46],[15,30,15,34],[18,39,18,40],[16,30,16,31],[16,32,16,33],[16,37,16,38],[16,35,16,36],[17,7,18,7],[18,12,18,16],[18,21,18,23],[16,1,16,8],[17,1,18,1],[17,2,18,2],[17,3,18,3],[17,4,18,4],[17,5,18,5],[17,6,18,6],[16,11,16,20],[16,21,16,27],[10,11,11,11],[10,14,11,14],[12,10,12,11],[12,21,12,22],[14,30,14,40],[10,10,11,10],[12,16,12,17],[10,15,11,15],[15,35,15,38],[15,39,15,40],[10,13,12,13],[14,1,14,2],[14,3,14,5],[10,7,12,7],[10,8,11,8],[10,9,11,9],[13,1,13,2],[13,3,13,5],[10,1,10,2],[10,3,10,5],[11,1,11,2],[11,3,11,5],[12,1,12,2],[12,3,12,5]]}
[0]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"General Project Totals",null,null,null,"Cooling Project Totals",null,null,null,null,null,null,null,null,null,"Heating Project Totals"]
[null,null,null,null,null,null,null,"Number of Units",null,"0 Units",null,"Chilled Water",null,"0 GPM","Primary Air Latent",null,"0 BTUH","Overall Capacity",null,"0 BTUH",null,"Hot Water",null,"0 GPM","Coil Capacity",null,"0 BTUH"]
[null,null,null,null,null,null,null,"Area",null,"0 ft2",null,"Avg Chilled Water ∆T",null,"0 °F","Secondary Air Sensible",null,"0 BTUH",null,null,null,null,"Avg Hot Water ∆T",null,"0 °F","Net Capacity",null,"0 BTUH"]
[null,null,null,null,null,null,null,"Primary Air",null,"0 CFM",null,"Primary Air Sensible",null,"0 BTUH","Net Sensible",null,"0 BTUH",null,null,null,null,"Primary Air Offset Capcity",null,"0 BTUH"]
[]
[null,"Project Name:",null,null,null,null,null,"Room Conditions","Dry Bulb","Relative Humidity","Dew Point","On-Coil Air Temp",null,"Primary Air Conditions","Dry Bulb","Relative Humidity","Wet Bulb","Dew Point",null,"Enter Water Temp","Entering Water","Propylene Glycol","Ethylene Gylcol",null,"Elevation"]
[null,"Project Number:"]
[null,"Version:",null,null,null,null,null,null,"°F","%","°F",null,null,null,"°F","%","°F",null,null,null,"°F","%",null,null,"ft"]
[null,"Date:",null,"2019-04-03",null,null,null,"Cooling",75,50,55.1,75,null,"Cooling",55,78,51.3,48.3,null,"Cooling",57,0,0,null,0]
[null,"Software Version:",null,1,null,null,null,"Heating",70,50,50.5,null,null,"Heating",75,50,62.6,55.1,null,"Heating",120,0,0,null,null,null,null,null,null,null,"Local Design Conditions"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Room Conditions",null,null,null,null,"Primary Air Conditions",null,null,null,"Entering Water"]
[null,"Active Chilled Beams",null,null,null,null,null,null,null,null,null,"Cooling Data Per Unit",null,null,null,null,null,null,null,null,null,"Heating Data Per Unit",null,null,null,null,null,null,null,null,"Cooling",null,"Heating",null,"Cooling","Cooling",null,"Heating",null,"Cooling","Heating","Sound Power Levels (No Attenuation)",null,null,null,null,null,"Velocity & Throw Data",null,null,"Throw"]
[null,"Unit Tag","Zone Name or Number","Number of Units","Model","Nozzle Config.","2 or 4 Pipe","Throw Direction","Model Length","Primary Air Pressure","Primary Airflow Rate","Supply Air Flow Rate","Primary Air Sensible","Primary Air Latent","Secondary Air Sensible","Net Unit Sensible","Total Capacity","Leaving Water Temp","Chilled Water Flow Rate","Water Pressure Drop","Supply Air Temp Out","Primary Air Offset Capacity","Coil Capacity","Net Unit Capacity","Leaving Water Temp","Heating Water Flow Rate","Water Pressure Drop","Supply Air Temp Out","Primary Air Inlet","Sound Level\nWith\n3 dB Atten.","Dry Bulb","Relative Humidity","Dry Bulb","Relative Humidity","On-Coil Air Temp","Dry Bulb","Relative Humidity","Dry Bulb","Relative Humidity","Entering Water","Entering Water","125 Hz","250 Hz","500 Hz","1000 Hz","2000 Hz","4000 Hz","Wall Airflow Velocity","Colliding Airflow Velocity","Isothermal Supply Air Temp","Isothermal\r\n\r\n(T150-100-50)"]
[null,null,null,null,null,null,null,null,"ft","Inch WC","CFM","CFM","BTUH",null,null,null,null,"°F","GPM","ft WC","°F","BTUH",null,null,"°F","GPM","ft WC","°F","Inch","NC","°F","%","°F","%","°F","°F","%","°F","%","°F",null,"dB",null,null,null,null,null,"FPM",null,"°F","ft"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]

{"sheet":"Throw Data","index":2,"n_rows":33,"n_cols":55,"rows_kept":33,"cut":false,"hidden":true,"merged":[[5,18,5,54],[32,18,32,54],[6,14,10,14],[6,15,10,15],[6,16,10,16],[5,13,5,15],[6,13,10,13],[11,13,11,14],[0,1,3,54],[6,11,10,11],[5,1,11,1],[5,2,11,2],[11,9,11,12],[5,9,5,12],[5,4,11,4],[6,12,10,12],[5,5,5,8],[6,6,10,6],[6,5,11,5],[6,7,10,7],[6,8,10,8],[6,9,10,9],[6,10,10,10],[5,3,11,3]]}
[14]
[]
[]
[]
[]
[null,"Unit Tag","Zone Name or Number","Number of Units","Grille Type and Direction","Selection Data",null,null,null,"Room Data",null,null,null,"Velocity Information",null,null,"Throw",null,"Dynamic Sample Beam Layout - Click a Unit Tag to Show Its Approximate Room Placement (Each Square = 1 ft)"]
[null,null,null,null,null,"Model","Model Length","Primary Air Pressure","Supply Airflow Rate","Beam Mounting Height or Room Height (H)","Distance From Beam to Wall (W)","Distance Between Beams (C)","Occupied Zone Height (Z)","Wall Airflow Velocity","Colliding Airflow Velocity","Isothermal Supply Air Temp","Isothermal\r\n\r\n(T150-100-50)",null,24,null,null,null,"* Out of Tolerance"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20]
[null,null,null,null,null,null,"ft","Inch WC","CFM","ft",null,null,null,"FPM",null,"°F","ft",null,19]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",75,"-",null,17]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definitions"]

{"sheet":"Statistics","index":3,"n_rows":21,"n_cols":53,"rows_kept":21,"cut":false,"hidden":true,"merged":[[15,41,15,52],[16,34,17,34],[16,39,16,40],[16,41,17,41],[16,35,16,38],[16,45,16,48],[16,49,16,52],[16,44,17,44],[16,43,17,43],[16,42,17,42],[18,31,18,33],[16,29,16,33],[15,34,15,40],[15,15,15,33],[16,15,18,15],[16,16,18,16],[16,17,17,17],[16,18,17,18],[16,19,17,19],[18,36,18,38],[18,24,18,28],[16,22,16,28],[16,21,17,21],[16,20,17,20],[15,14,18,14],[16,5,17,5],[16,6,17,6],[16,7,17,7],[16,8,17,8],[16,10,18,10],[16,11,18,11],[16,9,18,9],[16,12,17,12],[11,5,11,6],[5,9,5,11],[15,10,15,12],[15,5,15,9],[18,5,18,7],[8,9,8,10],[9,9,9,10],[10,9,10,10],[6,5,6,6],[9,5,9,6],[7,5,7,6],[10,5,10,6],[8,5,8,6],[0,1,3,52],[15,2,18,2],[15,3,18,3],[15,4,17,4],[15,1,18,1],[5,5,5,7],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[5,1,5,3],[10,1,10,2],[11,1,11,2],[6,9,6,10],[7,9,7,10],[12,5,12,6]]}
[]
[]
[]
[]
[]
[null,"General Project Totals",null,null,null,"Cooling Project Totals",null,null,null,"Heating Project Totals"]
[null,"Number of Groups",null,"1 Group",null,"Chilled Water",null,null,null,"Hot Water"]
[null,"Number of Zones",null,null,null,"Avg Chilled Water ∆T",null,null,null,"Avg Hot Water ∆T"]
[null,"Number of Units",null,null,null,"Primary Air Sensible",null,null,null,"Primary Air Offset Capacity"]
[null,"Area",null,null,null,"Primary Air Latent",null,null,null,"Coil Capacity"]
[null,"Primary Air",null,null,null,"Secondary Air Sensible",null,null,null,"Net Capacity"]
[null,"Length of Beams",null,null,null,"Net Sensible"]
[null,null,null,null,null,"Overall Capacity"]
[]
[]
[null,"Statistics Group","Unit Tag","Zone Name or Number","Area","Design Requirements",null,null,null,null,"Design Criteria",null,null,null,"Group Number","General Totals",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Area Averages",null,null,null,null,null,null,"Other Averages"]
[null,null,null,null,null,"Sensible Load","Latent Load","Heating Load","Min. Outside Air or Primary Airflow","Number of Units","Model","2 or 4 Pipe","Model Length",null,null,"Number of Zones","Number of Units","Area","Primary Air","Length of Beams","Max Primary Air Pressure Drop","Max Water Pressure Drop","Cooling Data",null,null,null,null,null,null,"Heating Data",null,null,null,null,"Primary Air / Area","Cooling Data",null,null,null,"Heating Data",null,"Primary Air / Unit","Primary Air / Unit Length","Area / Unit","Area / Unit Length","Cooling Data",null,null,null,"Heating Data"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water Flow Rate","Avg Chilled Water ∆T","Primary Air Sensible","Primary Air Latent","Secondary Air Sensible","Net Unit Sensible","Total Cooling Capacity","Hot Water Flow Rate","Avg Hot Water ∆T","Primary Air Offset","Heating Coil Capacity","Net Heating Capacity",null,"Chilled Water / Area","Net Sensible Cooling / Area","Latent Cooling / Area","Total Cooling / Area","Hot Water / Area","Total Heating / Area",null,null,null,null,"Chilled Water / Unit","Chilled Water / Unit Length","Sensible Cooling / Unit","Sensible Cooling / Unit Length","Hot Water / Unit","Hot Water / Unit Length","Total Heating / Unit","Total Heating / Unit Length"]
[null,null,null,null,"ft2","BTUH",null,null,"CFM",null,null,null,"ft",null,null,null,null,"ft2","CFM","ft","Inch WC","ft WC","GPM","°F","BTHU",null,null,null,null,"GPM","°F","BTHU",null,null,"CFM / ft2","GPM / ft2","BTUH / ft2",null,null,"GPM / ft2","BTUH / ft2","CFM / Unit","CFM / ft","ft2 / Unit","ft2 / ft","GPM / Unit","GPM / ft","BTUH / Unit","BTUH / ft","GPM / Unit","GPM / ft","BTUH / Unit","BTUH / ft"]
[]
[null,null,null,null,"-","-","-","-","-","-","-","-","-",null,"(blank)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]

{"sheet":"Backend Data","index":4,"n_rows":358,"n_cols":93,"rows_kept":358,"cut":false,"hidden":true,"merged":[]}
["Table_ACB40_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table_Coil_Types_4",null,null,null,null,"Table_Coil_Face_Area_4",null,null,"Table_Coil_Circuits_4",null,null,"Table_Initial_PD_4",null,null,null,null,null,null,null,null,null,null,null,null,null,"Table_Spigot_Shapes_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"Beam Name","Coil Name","Tube ID","Tube Area",null,"Coil Name, Length","Area",null,"Coil Name, Length, Pipe Count","<= H2O ∆P (C)",null,"Coil Name, Min Circuits","A","B","C","2","3","4","5","6","7","8","9","10",null,"Size","Area (square meters)",null,null,null,null,null,null,"Table_Auto_Selection_Menu_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table_Air_Turndown_4"]
[16,"TN",26,"TN",34,"TN",44,"TN",54,"TN",64,"TN",74,"TN",84,"TN",94,"TN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"44-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"64-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"74-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"84-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"94-TN"},null,"ACB40","CAL40",1.1887E-2,1.11E-4,null,"CAL40_2",0.11006100000000001,null,"CAL40_2_2",1,null,"CAL40_1",2368.2367760000002,1.817157122,-9.5740996999999994E-2,0.43,0.57999999999999996,0.72,0.86,1,1.1399999999999999,1.28,1.42,1.55,null,"4_Round",8.1069999999999996E-3,null,null,null,null,null,null,"Menu_CW_DT","Menu_HW_DT","Menu_Max_NU","Menu_Min_BL","Menu_Max_BL","Menu_NU_Check","Menu_BL_Check","Menu_TP_Check","Menu_PA_Check","Menu_CW_Check","Menu_HW_Check","Menu_Even_Unit_Check","Menu_Spigot_Check","Menu_PA_Row_Unit_Check","Menu_Spigot_Velocity","Menu_Latent_Airflow","Latent_Airflow_Check",null,"Turndown_10","Turndown_20","Turndown_30","Turndown_40","Turndown_50","Nozzle_Check","Active_Userform_Check"]
[26,"TN",34,"TN",42,"TN",54,"TN",64,"TN",78,"TN",88,"TN",100,"TN",112,"TN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"54-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"64-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"78-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"88-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"100-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"112-TN"},null,"ACB50","CAL40",1.1887E-2,1.11E-4,null,"CAL40_3",0.18747750000000002,null,"CAL40_3_2",1,null,"FM30_1",1652.029704,1.825528461,-9.1460582999999998E-2,0.73,0.87,1,1.2,1.4,null,null,null,null,null,"5_Round",1.2668E-2,null,null,null,null,null,null,0,0,20,2,8,false,false,false,false,false,false,false,false,"None",600,30,false,null,false,false,false,false,false,false,false]
[24,"UN",42,"TN",50,"TN",64,"TN",74,"TN",94,"TN",104,"TN",118,"TN",132,"TN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"42-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"50-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"64-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"74-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"94-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"104-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"118-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"132-TN"},null,"FMVBY","FM30",1.1887E-2,1.11E-4,null,"CAL40_4",0.26489400000000002,null,"CAL40_4_2",1,null,"ACB45_2",802.83864679999999,1.8377399999999999,-9.8900000000000002E-2,0.4,0.55000000000000004,0.7,0.85,1,1.1499999999999999,1.3,1.45,1.6,null,"6_Round",1.8241E-2,null,null,null,null,null,null,""]
[30,"UN",36,"UN",60,"TN",76,"TN",88,"TN",112,"TN",122,"TN",138,"TN",156,"TN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"60-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"76-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"88-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"112-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"122-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"138-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"156-TN"},null,"ACB35","FM30",1.1887E-2,1.11E-4,null,"CAL40_5",0.34237499999999998,null,"CAL40_5_2",1,null,"ACB3L_1",815.07425379999995,1.8227590149999999,-9.2172910999999996E-2,0.73,0.87,1,1.2,1.4,null,null,null,null,null,"8_Round",3.2428999999999999E-2,null,null,null,null,null,null,"Table_Header_Index_4"]
[24,"SN",42,"UN",70,"TN",64,"UN",102,"TN",128,"TN",142,"TN",160,"TN",180,"TN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"70-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"64-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"102-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"128-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"142-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"160-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"180-TN"},null,"HACB20","ACB20",1.1887E-2,1.11E-4,null,"CAL40_6",0.41985600000000001,null,"CAL40_6_2",1,null,"ACB20_2",721,1.91,-8.0500000000000002E-2,0.43,0.57999999999999996,0.72,0.86,1,1.1399999999999999,1.28,1.42,1.55,null,"10_Round",5.0671000000000001E-2,null,null,null,null,null,null,"UNIT TAG","ZONE NAME OR NUMBER","AREA","SENSIBLE LOAD","LATENT LOAD","HEATING LOAD","MIN. OUTSDIE AIR OR PRIMARY AIRFLOW","NUMBER OF UNITS","MODEL","2 OR 4 PIPE","MODEL LENGTH","TARGET PRIMARY AIR PRESSURE","PRIMARY AIRFLOW RATE","CHILLED WATER FLOW RATE","HEATING WATER FLOW RATE","SPIGOT SIZE","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16"]
[30,"SN",50,"UN",82,"TN",72,"UN",86,"UN",108,"UN",116,"UN",132,"UN",148,"UN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"30-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"50-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"82-TN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"72-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"86-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"108-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"116-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"132-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"148-UN"},null,"ACB20","ACB20",1.1887E-2,1.11E-4,null,"CAL40_7",0.497305,null,"CAL40_7_2",1,null,"ACB60_1",2961.1876699999998,1.816597477,-9.5726586000000002E-2,0.45,0.59,0.73,0.86,1,1.1399999999999999,1.28,1.41,1.55,null,"8_Elliptical",2.8257000000000001E-2,null,null,null,null,null,null,"UNIT TAG","ZONE NUMBER","AREA","NET UNIT SENSIBLE","PRIMARY AIR LATENT","NET UNIT CAPACITY","MIN OUTSIDE AIR OR PRIAMRY AIRFLOW","NUMBER OF UNITS","MODEL","2 OR 4 PIPE","MODEL LENGTH","PRIMARY AIR PRESSURE","PRIMARY AIRFLOW RATE","CHILLED WATER FLOW RATE","HEATING WATER FLOW RATE","SPIGOT SIZE",{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":"*UNIT*TAG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ZONE*NUMBER*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":"*AREA*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*UNIT*SENSIBLE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":"*PRIMARY*AIR*LATENT*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*NET*UNIT*CAPACITY*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*MIN*OUTSIDE*AIR*OR*PRIAMRY*AIRFLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":"*NUMBER*OF*UNITS*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":"*MODEL*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":"*2*OR*4*PIPE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":"*MODEL*LENGTH*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":"*PRIMARY*AIR*PRESSURE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":"*PRIMARY*AIRFLOW*RATE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*CHILLED*WATER*FLOW*RATE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*HEATING*WATER*FLOW*RATE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":"*SPIGOT*SIZE*"}]
[22,"MN",40,"SN",68,"UN",82,"UN",100,"UN",122,"UN",134,"UN",152,"UN",170,"UN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"68-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"82-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"100-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"122-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"134-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"152-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"170-UN"},null,"ACB30","FM30",1.1887E-2,1.11E-4,null,"CAL40_8",0.57475399999999999,null,"CAL40_8_2",1,null,"ACB25_1",2790,1.81,-0.11,0.45,0.59,0.73,0.86,1,1.1399999999999999,1.28,1.41,1.55,null,"4_Oval",5.8999999999999999E-3,null,null,null,null,null,null,"PLAN CODE","ZONE NAME","FT SQ","NET SENSIBLE COOLING","LATENT LOAD","NET UNIT HEATING","MIN FLOW","COUNT","UNIT TYPE","PIPE CONFIG","NOMINAL LENGTH","AIR PRESSURE","PRIMARY AIRFLOW","CHILLED WATER FLOW RATE","HEATING WATER FLOW RATE","SPIGOT DIAMETER",{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":"*PLAN*CODE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ZONE*NAME*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":"*FT*SQ*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*SENSIBLE*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":"*LATENT*LOAD*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*NET*UNIT*HEATING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*MIN*FLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":"*COUNT*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":"*UNIT*TYPE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":"*PIPE*CONFIG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":"*NOMINAL*LENGTH*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":"*AIR*PRESSURE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":"*PRIMARY*AIRFLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*CHILLED*WATER*FLOW*RATE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*HEATING*WATER*FLOW*RATE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":"*SPIGOT*DIAMETER*"}]
[24,"MN",44,"SN",78,"UN",64,"SN",78,"SN",138,"UN",152,"UN",170,"UN",192,"UN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"44-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"78-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"64-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"78-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"138-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"152-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"170-UN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"192-UN"},null,"FMLBY","FM30",1.1887E-2,1.11E-4,null,"CAL40_9",0.65223549999999997,null,"CAL40_9_2",1,null,"ACB44_1",2800,1.86,-0.104,1,null,1.29,null,null,null,null,null,null,null,"6_Oval",1.2149999999999999E-2,null,null,null,null,null,null,"TAG","ZONE ID",null,"NET COOLING TOTAL","LATENT COOLING","HEATING CAPACITY TOTAL","OUTSIDE FLOW","QUANTITY","UNIT TYPE","PIPING CONFIG","BEAM LENGTH","STATIC PRESSURE","AIRFLOW RATE","COLD WATER FLOW","HOT WATER FLOW","SPIGOT",{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":"*TAG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ZONE*ID*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*COOLING*TOTAL*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":"*LATENT*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*HEATING*CAPACITY*TOTAL*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*OUTSIDE*FLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":"*QUANTITY*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":"*UNIT*TYPE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":"*PIPING*CONFIG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":"*BEAM*LENGTH*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":"*STATIC*PRESSURE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":"*AIRFLOW*RATE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*COLD*WATER*FLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*HOT*WATER*FLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":"*SPIGOT*"}]
[28,"MN",48,"SN",58,"SN",70,"SN",88,"SN",104,"SN",116,"SN",132,"SN",148,"SN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"48-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"58-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"70-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"88-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"104-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"116-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"132-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"148-SN"},null,"FMTBY","FM30",1.1887E-2,1.11E-4,null,"CAL40_10",0.72971699999999995,null,"CAL40_10_2",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8_Oval",1.907E-2,null,null,null,null,null,null,"MARK","ROOM NUMBER",null,"NET TOTAL COOLING","LATENT","NET HEATING","MIN AIR","QUANTITIES","BEAM","COIL CONFIG","UNIT LENGTH","STATIC ","PRIMARY AIR","COOLING WATER FLOW","HEATING WATER GPM","INLET",{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":"*MARK*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ROOM*NUMBER*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*TOTAL*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":"*LATENT*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*NET*HEATING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*MIN*AIR*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":"*QUANTITIES*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":"*BEAM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":"*COIL*CONFIG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":"*UNIT*LENGTH*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":"*STATIC**"},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":"*PRIMARY*AIR*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*COOLING*WATER*FLOW*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*HEATING*WATER*GPM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":"*INLET*"}]
[30,"MN",36,"MN",64,"SN",78,"SN",100,"SN",116,"SN",128,"SN",146,"SN",164,"SN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"30-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"64-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"78-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"100-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"116-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"128-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"146-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"164-SN"},null,"ACB45","ACB45",8.8599999999999998E-3,6.1699999999999995E-5,null,"ACB20_2",0.11006100000000001,null,"CAL40_2_4",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10_Oval",3.4909999999999997E-2,null,null,null,null,null,null,"DESIG","ROOM NAME",null,"NET SENSIBLE LOAD","SENSIBLE COOLING LAT","TOTAL HEATING","OUTSIDE AIR","QTY",null,"PIPING CONFIG","LENGTH","MAX APD",null,"CHILLED WATER GPM","HOT WATER GPM",null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":"*DESIG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ROOM*NAME*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*SENSIBLE*LOAD*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*COOLING*LAT*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*TOTAL*HEATING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*OUTSIDE*AIR*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":"*QTY*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":"*PIPING*CONFIG*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":"*LENGTH*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":"*MAX*APD*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*CHILLED*WATER*GPM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*HOT*WATER*GPM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[34,"MN",40,"MN",72,"SN",88,"SN",112,"SN",128,"SN",142,"SN",162,"SN",182,"SN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"72-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"88-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"112-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"128-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"142-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"162-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"182-SN"},null,"ACB55","ACB45",8.8599999999999998E-3,6.1699999999999995E-5,null,"ACB20_3",0.18747750000000002,null,"CAL40_3_4",1,null,"Table_Pitch_Values_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROOM ID",null,"NET SENSIBLE LOAD",null,"NET CAPACITY","MIN CFM",null,null,"PIPE","MODEL SIZE",null,null,"COLD WATER GPM","HOT WATER",null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ROOM*ID*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*SENSIBLE*LOAD*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*NET*CAPACITY*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*MIN*CFM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":"*PIPE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":"*MODEL*SIZE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*COLD*WATER*GPM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*HOT*WATER*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[36,"MN",44,"MN",52,"MN",66,"MN",82,"MN",142,"SN",158,"SN",178,"SN",200,"SN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"142-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"158-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"178-SN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"200-SN"},null,"FMABY","FM30",1.1887E-2,1.11E-4,null,"ACB20_4",0.26489400000000002,null,"CAL40_4_4",1,null,"ACB3L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZONE",null,"SENSIBLE COOLING TOTAL",null,"NET HEATING","VENTILATION",null,null,null,null,null,null,"COLD WATER",null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ZONE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*COOLING*TOTAL*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*NET*HEATING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":"*VENTILATION*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":"*COLD*WATER*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
["","",48,"MN",56,"MN",72,"MN",92,"MN",102,"MN",114,"MN",130,"MN",146,"MN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"48-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"92-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"114-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"130-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"146-MN"},null,"ACB44","ACB44",1.1887E-2,1.11E-4,null,"ACB20_5",0.34412500000000001,null,"CAL40_5_4",1,null,22.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NUMBER",null,"SENSIBLE TOTAL COOLING",null,"HEATING CAPACITY",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*NUMBER*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*TOTAL*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*HEATING*CAPACITY*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
["","",52,"MN",62,"MN",80,"MN",100,"MN",110,"MN",124,"MN",140,"MN",160,"MN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"80-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"100-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"110-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"124-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"140-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"160-MN"},null,"ACB3L","ACB3L",1.1887E-2,1.11E-4,null,"ACB20_6",0.41985600000000001,null,"CAL40_6_4",1,null,24.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROOM",null,"SENSIBLE COOLING",null,"UNIT HEATING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*ROOM*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*UNIT*HEATING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
["","",56,"MN",66,"MN",88,"MN",108,"MN",122,"MN",136,"MN",154,"MN",174,"MN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"88-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"108-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"122-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"136-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"154-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"174-MN"},null,"ACB60","ACB60",1.1887E-2,1.11E-4,null,"ACB20_7",0.497305,null,"CAL40_7_4",1,null,28.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOOR",null,"SENSIBLE LOAD",null,"UNIT CAPACITY",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":"*FLOOR*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*LOAD*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":"*UNIT*CAPACITY*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
["","",62,"MN",72,"MN",96,"MN",118,"MN",132,"MN",146,"MN",166,"MN",188,"MN",{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"96-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"118-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"132-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"146-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"166-MN"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"188-MN"},null,"ACB10","FM30",1.1887E-2,1.11E-4,null,"ACB20_8",0.57475399999999999,null,"CAL40_8_4",1,null,33.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SENSIBLE TOTAL",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*TOTAL*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB35","FM30",1.1887E-2,1.11E-4,null,"ACB20_9",0.65223549999999997,null,"CAL40_9_4",1,null,40.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOTAL SENSIBLE",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*TOTAL*SENSIBLE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB40_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB40_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB40_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L","CAL40",1.1887E-2,1.11E-4,null,"ACB20_10",0.72971699999999995,null,"CAL40_10_4",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOTAL COOLING",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*TOTAL*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB5L","CAL40",1.1887E-2,1.11E-4,null,"FM30_2",0.14199999999999999,null,"ACB60_2_2",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NET COOLING",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*NET*COOLING*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB25","ACB25",1.1887E-2,1.11E-4,null,"FM30_3",0.19432199999999999,null,"ACB60_3_2",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COOLING LOAD",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*COOLING*LOAD*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FM30_4",0.24587000000000001,null,"ACB60_4_2",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COOLING LOAD SENSIBLE",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*COOLING*LOAD*SENSIBLE*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
["Table_ACB50_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FM30_5",0.32257999999999998,null,"ACB60_5_2",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SENSIBLE COIL",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":"*SENSIBLE*COIL*"},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,null,null,null,null,null,"FM30_6",0.39999899999999999,null,"ACB60_6_2",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[11,"UN",13,"UN",15,"UN",19,"UN",30,"TN",29,"UN",40,"TN",51,"TN",51,"TN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"11-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"13-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"15-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"19-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"30-TN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"29-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"40-TN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"51-TN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"51-TN"},null,null,null,null,null,null,"ACB45_2",4.7399999999999998E-2,null,"ACB60_7_2",1,null,"Table_Induction_Ratio_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[12,"SN",19,"UN",19,"UN",25,"UN",30,"UN",38,"UN",41,"UN",46,"UN",51,"UN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"12-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"19-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"25-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"38-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"41-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"46-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"51-UN"},null,null,null,null,null,null,"ACB45_3",7.8399999999999997E-2,null,"ACB60_8_2",1,null,"Beam Name, Nozzle, Pitch","A","B","Max Pressure 1","X0","X1","X2","X3","Max Pressure 2","Max ER","2","3","4","5","6","7","8","9","10","Min Pressure","Min ER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[10,"MN",17,"SN",24,"UN",33,"UN",39,"UN",46,"UN",53,"UN",57,"UN",65,"UN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"10-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"17-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"39-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"46-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"53-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"57-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"65-UN"},null,"Table_Nozzleplate_Length_4",null,null,null,null,"ACB45_4",0.1094,null,"ACB60_9_2",1,null,"ACB3L_UN_24.9",0,1.9,101,1.804,1.1000000000000001E-3,0,0,400,2.25,1,1,1,1,1,1,1,1,1,100,1.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[13,"MN",22,"SN",20,"SN",27,"SN",32,"SN",55,"UN",45,"SN",68,"UN",78,"UN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"13-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"27-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"32-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"55-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"45-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"68-UN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"78-UN"},null,"Beam Name, Length","Nozzleplate Length",null,null,null,"ACB45_5",0.14030000000000001,null,"ACB60_10_2",1,null,"ACB3L_SN_22.6",0.2072,0.60160000000000002,1000,2,0,0,0,2000,2,1,1,1,1,1,1,1,1,1,100,1.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[16,"MN",26,"SN",23,"SN",32,"SN",38,"SN",43,"SN",53,"SN",54,"SN",61,"SN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"23-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"32-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"38-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"43-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"53-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"54-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"61-SN"},null,"ACB40_2",15.077999999999999,null,null,null,"ACB45_6",0.17130000000000001,null,"ACB60_2_4",1,null,"ACB3L_MN_28.6",0.17369999999999999,0.6613,800,1.8,0,0,0,5000,1.8,1,1,1,1,1,1,1,1,1,1,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[18,"MN",20,"MN",27,"SN",37,"SN",44,"SN",50,"SN",61,"SN",62,"SN",69,"SN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"27-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"37-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"44-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"50-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"61-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"62-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"69-SN"},null,"ACB40_3",27.077999999999999,null,null,null,"ACB45_7",0.20230000000000001,null,"ACB60_3_4",1,null,"ACB3L_MN_24.9",0,1.3,25,1.2517,8.7000000000000001E-4,0,0,400,1.57,1,1,1,1,1,1,1,1,1,24,1.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,23,"MN",32,"SN",42,"SN",50,"SN",56,"SN",69,"SN",71,"SN",77,"SN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"23-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"56-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"69-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"71-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"77-SN"},null,"ACB40_4",39.078000000000003,null,null,null,"ACB45_8",0.23319999999999999,null,"ACB60_4_4",1,null,"ACB3L_MN_22.6",0.121,0.58919999999999995,800,1.4,0,0,0,5000,1.4,1,1,1,1,1,1,1,1,1,1,0.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,25,"MN",36,"SN",47,"SN",56,"SN",64,"SN",76,"SN",81,"SN",86,"SN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"36-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"47-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"56-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"64-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"76-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"81-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"86-SN"},null,"ACB40_5",51.078000000000003,null,null,null,"ACB45_9",0.26419999999999999,null,"ACB60_5_4",1,null,"ACB3L_TN_24.9",0,2.2000000000000002,6000,2.2000000000000002,0,0,0,7000,2.2000000000000002,1,1,1,1,1,1,1,1,1,5000,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,28,"MN",26,"MN",35,"MN",41,"MN",47,"MN",56,"MN",91,"SN",95,"SN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"47-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"91-SN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"95-SN"},null,"ACB40_6",63.084000000000003,null,null,null,"ACB45_10",0.29520000000000002,null,"ACB60_6_4",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,29,"MN",38,"MN",46,"MN",52,"MN",61,"MN",67,"MN",70,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"61-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"67-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"70-MN"},null,"ACB40_7",null,null,null,null,"ACB3L_2",7.0999999999999994E-2,null,"ACB60_7_4",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,32,"MN",41,"MN",50,"MN",57,"MN",66,"MN",74,"MN",76,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"57-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"76-MN"},null,"ACB40_8",87,null,null,null,"ACB3L_3",9.7160999999999997E-2,null,"ACB60_8_4",1,null,"Table_Octave_Coefs_4",null,null,null,null,null,"Table_Octave_Factors_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,35,"MN",45,"MN",55,"MN",63,"MN",72,"MN",81,"MN",83,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"63-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"81-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"83-MN"},null,"ACB40_9",null,null,null,null,"ACB3L_4",0.122935,null,"ACB60_9_4",1,null,"Octave, Nozzle","A","B","C","D",null,"Model","125","250","500","1000","2000","4000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,38,"MN",48,"MN",59,"MN",68,"MN",78,"MN",88,"MN",91,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"48-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"59-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"68-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"78-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"88-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"91-MN"},null,"ACB40_10",111.09699999999999,null,null,null,"ACB3L_5",0.16128999999999999,null,"ACB60_10_4",1,null,125,1.63789463851901E-2,1.1943340921483401,11.374452439232901,0.15578751141125299,null,"ACB40",1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table_Header_Index_4[[#This Row],[UNIT TAG]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[UNIT TAG]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[ZONE NAME OR NUMBER]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[AREA]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[AREA]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SENSIBLE LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[LATENT LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[LATENT LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING LOAD]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING LOAD]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MIN. OUTSDIE AIR OR PRIMARY AIRFLOW]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[NUMBER OF UNITS]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[2 OR 4 PIPE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[MODEL LENGTH]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[MODEL LENGTH]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[TARGET PRIMARY AIR PRESSURE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[PRIMARY AIRFLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[CHILLED WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[HEATING WATER FLOW RATE]],\" \",\"*\")&\"*\")","v":""},{"$f":"IF(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]]=\"\",\"\",\"*\"&SUBSTITUTE(Table_Header_Index_4[[#This Row],[SPIGOT SIZE]],\" \",\"*\")&\"*\")","v":""}]
[null,null,null,null,40,"MN",51,"MN",63,"MN",74,"MN",84,"MN",95,"MN",100,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"51-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"63-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"84-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"95-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"100-MN"},null,"ACB50_2",15.077999999999999,null,null,null,"ACB3L_6",0.2,null,"FM30_2_2",1,null,250,3.4718655908351002,0.36933484548349499,0.134923327817767,0.98096618805452396,null,"ACB50",1,1,1,1,1,1]
[null,null,null,null,42,"MN",55,"MN",68,"MN",79,"MN",91,"MN",103,"MN",113,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"55-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"68-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"79-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"91-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"103-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"113-MN"},null,"ACB50_3",27.077999999999999,null,null,null,"ACB60_2",0.13757625000000001,null,"FM30_3_2",1,null,500,-68.652988790242205,8.19586630527259,13.4762586495519,null,null,"ACB45",1,1,1,1,1,1]
[null,null,null,null,45,"MN",58,"MN",72,"MN",85,"MN",98,"MN",110,"MN",126,"MN",{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"58-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"85-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"98-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"110-MN"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"126-MN"},null,"ACB50_4",39.078000000000003,null,null,null,"ACB60_4",0.33111750000000001,null,"FM30_4_2",1,null,1000,-104.06108399574499,13.2937688161268,14.860994269476601,null,null,"ACB55",1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,"Table_Schedule_Creation_4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB50_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB50_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB50_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB50_5",51.078000000000003,null,null,null,"ACB60_6",0.52482000000000006,null,"FM30_5_2",1,null,2000,-99.231651007638504,16.401605819321201,9.4223811103185806,null,null,"ACB60",1.3,1.3,1.3,1.3,1.3,1.3,null,null,null,null,null,null,null,null,null,"Cooling","Heating","Local","Totals","Sound","Velocity","Throw","Create"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB50_6",63.084000000000003,null,null,null,"ACB60_8",0.71844249999999998,null,"FM30_6_2",1,null,4000,-108.95396768456099,19.255284536185201,7.5593536855150001,null,null,"ACB4L",1.2,1.2,1.2,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,true,true,false,false,false,false,false,true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB50_7",null,null,null,null,"ACB60_10",0.91214624999999994,null,"FM30_2_4",1,null,null,null,null,null,null,null,"ACB5L",1.2,1.2,1.2,1.2,1.2,1.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB50_8",87,null,null,null,"ACB44_2",0.12903999999999999,null,"FM30_3_4",1,null,null,null,null,null,null,null,"ACB10",1.2,1.2,1.2,1.2,1.2,1.2]
["Table_FMVBY_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB50_9",null,null,null,null,"ACB44_4",0.28391,null,"FM30_4_4",1,null,"Table_ACB44_Equiv_PA_4",null,null,null,null,null,"ACB20",1.2,1.2,1.2,1.2,1.2,1.2]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"ACB50_10",111.09699999999999,null,null,null,"ACB25_2",0.140321,null,"FM30_5_4",1,null,"Nozzle","Equiv PA",null,null,null,null,"ACB44",1.2,1.2,1.2,1.2,1.2,1.2]
[16,"SN",20,"UN",32,"TN",41,"TN",49,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-TN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-TN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-TN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMVBY_2",22.187999999999999,null,null,null,"ACB25_4",0.29515799999999998,null,"FM30_6_4",1,null,"38-TN",9.94,null,null,null,null,"FMLBY",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[18,"SN",24,"UN",29,"UN",36,"UN",42,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMVBY_3",30.297999999999998,null,null,null,"ACB25_6",0.44999499999999998,null,"ACB45_2_2",2,null,"38-UN",13.82,null,null,null,null,"FMTBY",1.4,1.4,1.4,1.4,1.4,1.4]
[21,"SN",20,"SN",34,"UN",42,"UN",48,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMVBY_4",38.298000000000002,null,null,null,"ACB25_8",0.60483200000000004,null,"ACB45_4_2",2,null,"48-UN",17.62,null,null,null,null,"FMVBY",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[16,"MN",22,"SN",26,"SN",33,"SN",54,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-UN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMVBY_5",50.177999999999997,null,null,null,null,null,null,"ACB45_6_2",2,null,"64-UN",23.75,null,null,null,null,"ACB30",1.2,1.2,1.2,1.2,1.2,1.2]
[18,"MN",25,"SN",30,"SN",36,"SN",43,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMVBY_6",62.177999999999997,null,null,null,null,null,null,"ACB45_8_2",2,null,"56-SN",30.2,null,null,null,null,"ACB25",1.2,1.2,1.2,1.2,1.2,1.2]
[20,"MN",19,"MN",34,"SN",41,"SN",49,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB45_2",null,null,null,null,null,null,null,"ACB45_10_2",2,null,"64-SN",34.67,null,null,"I put this in",">--->","ACB35",1.2,1.2,1.2,1.2,1.2,1.2]
[22,"MN",21,"MN",25,"MN",46,"SN",55,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"21-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB45_4",39.078000000000003,null,null,null,null,null,null,"ACB45_2_4",2,null,"72-SN",39.14,null,null,"I put this in",">--->","ACB3L",1.2,1.2,1.2,1.2,1.2,1.2]
[24,"MN",24,"MN",28,"MN",34,"MN",41,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"34-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB45_6",63.084000000000003,null,null,null,null,null,null,"ACB45_4_4",2,null,"82-SN",44.7]
[26,"MN",26,"MN",35,"MN",38,"MN",45,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"45-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB45_8",87,null,null,null,null,null,null,"ACB45_6_4",2,null,"90-SN",49.17]
["","",29,"MN",31,"MN",41,"MN",50,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"29-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB45_10",111.09699999999999,null,null,null,null,null,null,"ACB45_8_4",2,null,"98-SN",53.64]
["","",32,"MN",38,"MN",46,"MN",55,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB55_2",null,null,null,null,null,null,null,"ACB45_10_4",2,null,"74-MN",60.55]
["","",35,"MN",41,"MN",50,"MN",60,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB55_4",39.078000000000003,null,null,null,null,null,null,"ACB3L_2_2",1,null,"82-MN",67.28]
["","","","",44,"MN",53,"MN",65,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB55_6",63.084000000000003,null,null,null,null,null,null,"ACB3L_3_2",1,null,"90-MN",74.010000000000005]
["","","","","","",57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB55_8",87,null,null,null,null,null,null,"ACB3L_4_2",1,null,"98-MN",80.739999999999995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMVBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMVBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB55_10",111.09699999999999,null,null,null,null,null,null,"ACB3L_5_2",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FMLBY_2",22.187999999999999,null,null,null,null,null,null,"ACB3L_6_2",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FMLBY_3",30.297999999999998,null,null,null,null,null,null,"ACB20_2_2",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FMLBY_4",38.298000000000002,null,null,null,null,null,null,"ACB20_3_2",2]
["Table_FMLBY_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FMLBY_5",50.177999999999997,null,null,null,null,null,null,"ACB20_4_2",2]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"FMLBY_6",62.177999999999997,null,null,null,null,null,null,"ACB20_5_2",2]
[16,"SN",20,"UN",32,"TN",41,"TN",49,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-TN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-TN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-TN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB10_2",22.187999999999999,null,null,null,null,null,null,"ACB20_6_2",2]
[18,"SN",24,"UN",29,"UN",36,"UN",42,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB10_3",30.297999999999998,null,null,null,null,null,null,"ACB20_7_2",2]
[21,"SN",20,"SN",34,"UN",42,"UN",48,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB10_4",38.298000000000002,null,null,null,null,null,null,"ACB20_8_2",2]
[16,"MN",22,"SN",26,"SN",33,"SN",54,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-UN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB10_5",50.177999999999997,null,null,null,null,null,null,"ACB20_9_2",2]
[18,"MN",25,"SN",30,"SN",36,"SN",43,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB10_6",62.177999999999997,null,null,null,null,null,null,"ACB20_10_2",2]
[20,"MN",19,"MN",34,"SN",41,"SN",49,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB30_2",22.187999999999999,null,null,null,null,null,null,"ACB20_2_4",2]
[22,"MN",21,"MN",25,"MN",46,"SN",55,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"21-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB30_3",30.297999999999998,null,null,null,null,null,null,"ACB20_3_4",2]
[24,"MN",24,"MN",28,"MN",34,"MN",41,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"34-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB30_4",38.298000000000002,null,null,null,null,null,null,"ACB20_4_4",2]
[26,"MN",26,"MN",35,"MN",38,"MN",45,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"45-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB30_5",50.177999999999997,null,null,null,null,null,null,"ACB20_5_4",2]
[null,null,29,"MN",31,"MN",41,"MN",50,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"29-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB30_6",62.177999999999997,null,null,null,null,null,null,"ACB20_6_4",2]
[null,null,32,"MN",38,"MN",46,"MN",55,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB35_2",22.187999999999999,null,null,null,null,null,null,"ACB20_7_4",2]
[null,null,35,"MN",41,"MN",50,"MN",60,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB35_3",30.297999999999998,null,null,null,null,null,null,"ACB20_8_4",2]
[null,null,"","",44,"MN",53,"MN",65,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB35_4",38.298000000000002,null,null,null,null,null,null,"ACB20_9_4",2]
[null,null,null,null,"","",57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB35_5",50.177999999999997,null,null,null,null,null,null,"ACB20_10_4",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB35_6",62.177999999999997,null,null,null,null,null,null,"ACB44_2_2",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMLBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMLBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB3L_2",22.187999999999999,null,null,null,null,null,null,"ACB44_4_2",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB3L_3",30.297999999999998,null,null,null,null,null,null,"ACB44_2_4",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB3L_4",38.298000000000002,null,null,null,null,null,null,"ACB44_4_4",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB3L_5",50.177999999999997,null,null,null,null,null,null,"ACB25_2_2",1]
["Table_FMTBY_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB3L_6",62.177999999999997,null,null,null,null,null,null,"ACB25_4_2",1]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"FMTBY_2",22.187999999999999,null,null,null,null,null,null,"ACB25_6_2",1]
[16,"SN",20,"UN",32,"TN",41,"TN",49,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-TN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-TN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-TN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMTBY_3",30.297999999999998,null,null,null,null,null,null,"ACB25_8_2",1]
[18,"SN",24,"UN",29,"UN",36,"UN",42,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMTBY_4",38.298000000000002,null,null,null,null,null,null,"ACB25_2_4",1]
[21,"SN",20,"SN",34,"UN",42,"UN",48,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMTBY_5",50.177999999999997,null,null,null,null,null,null,"ACB25_4_4",1]
[16,"MN",22,"SN",26,"SN",33,"SN",54,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-UN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"FMTBY_6",62.177999999999997,null,null,null,null,null,null,"ACB25_6_4",1]
[18,"MN",25,"SN",30,"SN",36,"SN",43,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB60_2",28.21,null,null,null,null,null,null,"ACB25_8_4",1]
[20,"MN",19,"MN",34,"SN",41,"SN",49,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB60_4",40.21]
[22,"MN",21,"MN",25,"MN",46,"SN",55,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"21-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB60_6",64.209999999999994]
[24,"MN",24,"MN",28,"MN",34,"MN",41,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"34-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB60_8",88.21]
[26,"MN",26,"MN",35,"MN",38,"MN",45,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"45-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB60_10",112.21]
[null,null,29,"MN",31,"MN",41,"MN",50,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"29-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB20_2",16.5]
[null,null,32,"MN",38,"MN",46,"MN",55,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB20_3",28.5]
[null,null,35,"MN",41,"MN",50,"MN",60,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB20_4",40.5]
[null,null,"","",44,"MN",53,"MN",65,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB20_5",52.5]
[null,null,null,null,"","",57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB20_6",64.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_FMTBY_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_FMTBY_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB20_7",76.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB20_8",88.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB20_9",100.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB20_10",112.5]
["Table_ACB10_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB44_2",40]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"ACB44_4",88]
[16,"SN",20,"UN",32,"TN",41,"TN",49,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-TN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-TN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-TN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_2",15.077999999999999]
[18,"SN",24,"UN",29,"UN",36,"UN",42,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_3",27.077999999999999]
[21,"SN",20,"SN",34,"UN",42,"UN",48,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_4",39.078000000000003]
[16,"MN",22,"SN",26,"SN",33,"SN",54,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-UN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_5",51.078000000000003]
[18,"MN",25,"SN",30,"SN",36,"SN",43,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_6",63.084000000000003]
[20,"MN",19,"MN",34,"SN",41,"SN",49,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_7"]
[22,"MN",21,"MN",25,"MN",46,"SN",55,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"21-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_8",87]
[24,"MN",24,"MN",28,"MN",34,"MN",41,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_9"]
[26,"MN",26,"MN",35,"MN",38,"MN",45,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB4L_10",111.09699999999999]
[null,null,29,"MN",31,"MN",41,"MN",50,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"29-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB5L_2",15.077999999999999]
[null,null,32,"MN",38,"MN",46,"MN",55,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB5L_3",27.077999999999999]
[null,null,35,"MN",41,"MN",50,"MN",60,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB5L_4",39.078000000000003]
[null,null,"","",44,"MN",53,"MN",65,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB5L_5",51.078000000000003]
[null,null,null,null,"","",57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB5L_6",63.084000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB10_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB10_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB10_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"ACB5L_7"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB5L_8",87]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB5L_9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB5L_10",111.09699999999999]
["Table_ACB20_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB25_2",21.937999999999999]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"ACB25_4",45.938000000000002]
[16,"TN",28,"TN",38,"TN",48,"TN",58,"TN",70,"TN",80,"TN",90,"TN",100,"TN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"28-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"48-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"58-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"70-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"80-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"90-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"100-TN"},null,"ACB25_6",69.938000000000002]
[18,"UN",34,"TN",48,"TN",56,"TN",68,"TN",82,"TN",94,"TN",106,"TN",118,"TN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"48-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"56-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"68-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"82-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"94-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"106-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"118-TN"},null,"ACB25_8",93.938000000000002]
[16,"SN",30,"UN",42,"UN",48,"UN",80,"TN",70,"UN",82,"UN",90,"UN",102,"UN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"48-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"80-TN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"70-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"82-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"90-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"102-UN"}]
[20,"SN",36,"UN",50,"UN",56,"UN",66,"UN",82,"UN",96,"UN",106,"UN",122,"UN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"50-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"56-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"66-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"82-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"96-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"106-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"122-UN"}]
[24,"SN",30,"SN",40,"SN",66,"UN",78,"UN",96,"UN",110,"UN",124,"UN",140,"UN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"30-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"78-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"96-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"110-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"124-UN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"140-UN"}]
[20,"MN",34,"SN",46,"SN",52,"SN",62,"SN",74,"SN",86,"SN",98,"SN",112,"SN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"46-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"62-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"74-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"86-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"112-SN"}]
[22,"MN",40,"SN",52,"SN",60,"SN",70,"SN",86,"SN",98,"SN",112,"SN",128,"SN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"52-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"60-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"70-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"86-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"112-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"128-SN"}]
[24,"MN",44,"SN",58,"SN",68,"SN",82,"SN",98,"SN",112,"SN",128,"SN",144,"SN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"44-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"58-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"68-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"82-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"112-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"128-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"144-SN"}]
[28,"MN",48,"SN",64,"SN",78,"SN",92,"SN",110,"SN",124,"SN",144,"SN",162,"SN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"48-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"64-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"78-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"92-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"110-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"124-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"144-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"162-SN"}]
[30,"MN",36,"MN",46,"MN",88,"SN",104,"SN",124,"SN",140,"SN",162,"SN",182,"SN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"30-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"88-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"104-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"124-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"140-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"162-SN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"182-SN"}]
[34,"MN",40,"MN",50,"MN",66,"MN",78,"MN",92,"MN",104,"MN",120,"MN",134,"MN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"78-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"92-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"104-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"120-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"134-MN"}]
[36,"MN",44,"MN",54,"MN",74,"MN",86,"MN",102,"MN",114,"MN",132,"MN",150,"MN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"54-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"86-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"114-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"132-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"150-MN"}]
["","",48,"MN",58,"MN",82,"MN",94,"MN",112,"MN",126,"MN",146,"MN",166,"MN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"48-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"58-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"94-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"112-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"126-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"146-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"166-MN"},null,"Table_Octave_Nozzle_4"]
["","",52,"MN",62,"MN",90,"MN",106,"MN",122,"MN",138,"MN",160,"MN",180,"MN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"90-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"106-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"122-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"138-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"160-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"180-MN"},null,"Octave_Nozzle","Nozzle_A","Nozzle_B","Plenum_A","Plenum_B"]
["","",56,"MN",66,"MN",98,"MN",118,"MN",134,"MN",150,"MN",174,"MN",198,"MN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"98-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"118-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"134-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"150-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"174-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"198-MN"},null,"125_MN",8.7499999999999994E-2,5.6997,0.20569999999999999,16.846]
["","",62,"MN",72,"MN",106,"MN",132,"MN",146,"MN",164,"MN",188,"MN",214,"MN",{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"106-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"132-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"146-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"164-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"188-MN"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"214-MN"},null,"250_MN",7.1599999999999997E-2,10.478999999999999,0.24779999999999999,17.038]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"500_MN",8.43E-2,5.1966000000000001,0.3397,6.7291999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB20_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB20_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB20_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"1000_MN",4.3499999999999997E-2,22.832999999999998,0.35549999999999998,-3.7732000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2000_MN",8.5699999999999998E-2,12.843,0.1694,7.0717999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4000_MN",0.12690000000000001,2.3189000000000002,7.0599999999999996E-2,11.503]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125_SN",4.5999999999999999E-2,22.414999999999999,0.20569999999999999,16.846]
["Table_ACB30_Nozzle_4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"250_SN",6.7100000000000007E-2,18.93,0.24779999999999999,17.038]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C",null,"500_SN",9.7000000000000003E-2,10.519,0.3397,6.7291999999999996]
[16,"SN",20,"UN",32,"TN",41,"TN",49,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-TN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-TN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-TN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"1000_SN",0.1031,6.6566999999999998,0.35549999999999998,-3.7732000000000001]
[18,"SN",24,"UN",29,"UN",36,"UN",42,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"2000_SN",0.104,5.6401000000000003,0.1694,7.0717999999999996]
[21,"SN",20,"SN",34,"UN",42,"UN",48,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"4000_SN",0.1135,1.948,7.0599999999999996E-2,11.503]
[16,"MN",22,"SN",26,"SN",33,"SN",54,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-UN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"125_UN",1.6299999999999999E-2,23.343,0.20569999999999999,16.846]
[18,"MN",25,"SN",30,"SN",36,"SN",43,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"250_UN",4.9099999999999998E-2,13.856999999999999,0.24779999999999999,17.038]
[20,"MN",19,"MN",34,"SN",41,"SN",49,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"500_UN",8.4199999999999997E-2,5.4547999999999996,0.3397,6.7291999999999996]
[22,"MN",21,"MN",25,"MN",46,"SN",55,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"21-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"1000_UN",8.5900000000000004E-2,4.5682,0.35549999999999998,-3.7732000000000001]
[24,"MN",24,"MN",28,"MN",34,"MN",41,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"2000_UN",0.10580000000000001,1.8732,0.1694,7.0717999999999996]
[26,"MN",26,"MN",35,"MN",38,"MN",45,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"4000_UN",5.8599999999999999E-2,9.9515999999999991,7.0599999999999996E-2,11.503]
[null,null,29,"MN",31,"MN",41,"MN",50,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"29-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"125_TN",3.8800000000000001E-2,16.169,0.20569999999999999,16.846]
[null,null,32,"MN",38,"MN",46,"MN",55,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"250_TN",5.67E-2,12.805999999999999,0.24779999999999999,17.038]
[null,null,35,"MN",41,"MN",50,"MN",60,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"500_TN",8.5300000000000001E-2,4.7500999999999998,0.3397,6.7291999999999996]
[null,null,null,"",44,"MN",53,"MN",65,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"1000_TN",9.3799999999999994E-2,3.7263000000000002,0.35549999999999998,-3.7732000000000001]
[null,null,null,null,null,null,57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"2000_TN",0.09,4.4753999999999996,0.1694,7.0717999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB30_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB30_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB30_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"},null,"4000_TN",0.1012,0.12640000000000001,7.0599999999999996E-2,11.503]
[]
[]
[]
["Table_ACB35_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[16,"SN",20,"UN",32,"TN",41,"TN",49,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"32-TN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-TN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-TN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[18,"SN",24,"UN",29,"UN",36,"UN",42,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[21,"SN",20,"SN",34,"UN",42,"UN",48,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[16,"MN",22,"SN",26,"SN",33,"SN",54,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"26-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-UN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[18,"MN",25,"SN",30,"SN",36,"SN",43,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[20,"MN",19,"MN",34,"SN",41,"SN",49,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[22,"MN",21,"MN",25,"MN",46,"SN",55,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"21-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[24,"MN",24,"MN",28,"MN",34,"MN",41,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[26,"MN",26,"MN",35,"MN",38,"MN",45,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,29,"MN",31,"MN",41,"MN",50,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"29-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,32,"MN",38,"MN",46,"MN",55,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,35,"MN",41,"MN",50,"MN",60,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,"","",44,"MN",53,"MN",65,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,"","",57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB35_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB35_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB35_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
["Table_ACB45_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[28,"TN",50,"TN",70,"TN",90,"TN",112,"TN",132,"TN",154,"TN",174,"TN",196,"TN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"50-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"70-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"90-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"112-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"132-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"154-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"174-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"196-TN"}]
[30,"UN",62,"TN",80,"TN",104,"TN",128,"TN",150,"TN",176,"TN",198,"TN",222,"TN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"80-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"104-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"128-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"150-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"176-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"198-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"222-TN"}]
[28,"SN",52,"UN",90,"TN",116,"TN",142,"TN",170,"TN",196,"TN",222,"TN",250,"TN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"52-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"90-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"116-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"142-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"170-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"196-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"222-TN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"250-TN"}]
[34,"SN",62,"UN",76,"UN",90,"UN",112,"UN",138,"UN",154,"UN",174,"UN",196,"UN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"34-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"76-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"90-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"112-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"138-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"154-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"174-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"196-UN"}]
[28,"MN",50,"SN",90,"UN",100,"UN",126,"UN",152,"UN",176,"UN",198,"UN",224,"UN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"50-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"90-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"100-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"126-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"152-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"176-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"198-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"224-UN"}]
[32,"MN",62,"SN",70,"SN",116,"UN",142,"UN",170,"UN",196,"UN",222,"UN",250,"UN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"70-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"116-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"142-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"170-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"196-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"222-UN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"250-UN"}]
[36,"MN",50,"MN",80,"SN",90,"SN",112,"SN",132,"SN",154,"SN",174,"SN",196,"SN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"80-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"90-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"112-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"132-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"154-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"174-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"196-SN"}]
[null,null,54,"MN",90,"SN",102,"SN",126,"SN",142,"SN",174,"SN",196,"SN",224,"SN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"54-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"90-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"102-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"126-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"142-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"174-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"196-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"224-SN"}]
[null,null,58,"MN",70,"MN",116,"SN",142,"SN",156,"SN",196,"SN",222,"SN",250,"SN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"58-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"70-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"116-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"142-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"156-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"196-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"222-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"250-SN"}]
[null,null,62,"MN",78,"MN",90,"MN",112,"MN",170,"SN",154,"MN",174,"MN",196,"MN",{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"78-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"90-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"112-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"170-SN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"154-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"174-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"196-MN"}]
[null,null,null,null,86,"MN",100,"MN",126,"MN",132,"MN",174,"MN",196,"MN",null,null,{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"86-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"100-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"126-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"132-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"174-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"196-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,142,"MN",142,"MN",null,null,null,null,null,null,{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"142-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"142-MN"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB45_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB45_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB45_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
["Table_ACB55_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[14,"TN",25,"TN",35,"TN",45,"TN",56,"TN",66,"TN",77,"TN",87,"TN",98,"TN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"14-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"45-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"56-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"66-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"77-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"87-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"98-TN"}]
[17,"UN",25,"UN",45,"TN",51,"TN",63,"TN",79,"TN",88,"TN",98,"TN",108,"TN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"17-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"45-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"51-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"63-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"79-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"88-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"98-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"108-TN"}]
[17,"SN",31,"UN",41,"UN",58,"TN",71,"TN",67,"UN",98,"TN",111,"TN",125,"TN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"17-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"31-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"58-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"67-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"98-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"111-TN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"125-TN"}]
[14,"MN",26,"SN",35,"SN",50,"UN",61,"UN",77,"UN",77,"UN",87,"UN",102,"UN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"14-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"61-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"77-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"77-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"87-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"102-UN"}]
[18,"MN",31,"SN",40,"SN",58,"UN",71,"UN",85,"UN",88,"UN",99,"UN",112,"UN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"31-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"58-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"85-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"88-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"99-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"112-UN"}]
[null,null,25,"MN",45,"SN",45,"SN",56,"SN",66,"SN",98,"UN",111,"UN",125,"UN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"45-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"45-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"56-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"66-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"98-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"111-UN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"125-UN"}]
[null,null,28,"MN",35,"MN",52,"SN",63,"SN",75,"SN",77,"SN",87,"SN",98,"SN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"63-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"75-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"77-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"87-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"98-SN"}]
[null,null,31,"MN",38,"MN",58,"SN",71,"SN",85,"SN",84,"SN",99,"SN",112,"SN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"58-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"85-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"84-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"99-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"112-SN"}]
[null,null,null,null,41,"MN",45,"MN",56,"MN",66,"MN",91,"SN",111,"SN",125,"SN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"91-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"111-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"125-SN"}]
[null,null,null,null,45,"MN",52,"MN",60,"MN",72,"MN",98,"SN",87,"MN",98,"MN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"87-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"98-MN"}]
[null,null,null,null,null,null,58,"MN",65,"MN",79,"MN",77,"MN",98,"MN",106,"MN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"58-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"79-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"77-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"98-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"106-MN"}]
[null,null,null,null,null,null,null,null,71,"MN",85,"MN",84,"MN",111,"MN",116,"MN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"85-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"84-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"111-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"116-MN"}]
[null,null,null,null,null,null,null,null,null,null,null,null,91,"MN",null,null,125,"MN",{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"91-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"125-MN"}]
[null,null,null,null,null,null,null,null,null,null,null,null,98,"MN",null,null,null,null,{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"98-MN"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB55_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB55_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB55_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
["Table_ACB3L_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[24,"TN",32,"TN",40,"TN",52,"TN",64,"TN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-TN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-TN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-TN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-TN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"64-TN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[24,"UN",32,"UN",40,"UN",52,"UN",64,"UN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-UN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-UN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-UN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"64-UN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[26,"SN",35,"SN",44,"SN",57,"SN",71,"SN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-SN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-SN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-SN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-SN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-SN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[21,"MN",28,"MN",35,"MN",46,"MN",56,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[24,"MN",32,"MN",40,"MN",52,"MN",64,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"64-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[26,"MN",35,"MN",44,"MN",57,"MN",71,"MN",null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"57-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"71-MN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,53,"SN",null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"53-SN"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB3L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB3L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
["Table_ACB60_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[16,"TN",26,"TN",34,"TN",42,"TN",50,"TN",60,"TN",68,"TN",76,"TN",84,"TN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"42-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"50-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"60-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"68-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"76-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"84-TN"}]
[18,"UN",34,"TN",42,"TN",52,"TN",60,"TN",70,"TN",80,"TN",90,"TN",100,"TN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"60-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"70-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"80-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"90-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"100-TN"}]
[16,"SN",30,"UN",50,"TN",62,"TN",70,"TN",82,"TN",94,"TN",104,"TN",116,"TN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"50-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"62-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"70-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"82-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"94-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"104-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"116-TN"}]
[20,"SN",36,"UN",42,"UN",52,"UN",82,"TN",96,"TN",110,"TN",120,"TN",134,"TN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"82-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"96-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"110-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"120-TN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"134-TN"}]
[16,"MN",30,"SN",50,"UN",60,"UN",68,"UN",80,"UN",90,"UN",98,"UN",110,"UN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"30-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"50-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"60-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"68-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"80-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"90-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"98-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"110-UN"}]
[20,"MN",34,"SN",40,"SN",68,"UN",78,"UN",92,"UN",102,"UN",112,"UN",126,"UN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"68-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"78-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"92-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"102-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"112-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"126-UN"}]
[22,"MN",40,"SN",46,"SN",52,"SN",90,"UN",104,"UN",116,"UN",128,"UN",144,"UN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"46-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"52-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"90-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"104-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"116-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"128-UN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"144-UN"}]
[null,null,30,"MN",52,"SN",58,"SN",70,"SN",80,"SN",90,"SN",98,"SN",110,"SN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"30-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"52-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"58-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"70-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"80-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"90-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"110-SN"}]
[null,null,34,"MN",40,"MN",66,"SN",80,"SN",90,"SN",102,"SN",110,"SN",124,"SN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"80-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"90-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"102-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"110-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"124-SN"}]
[null,null,38,"MN",46,"MN",74,"SN",90,"SN",100,"SN",114,"SN",124,"SN",138,"SN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"74-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"90-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"100-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"114-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"124-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"138-SN"}]
[null,null,null,null,50,"MN",54,"MN",66,"MN",74,"MN",126,"SN",138,"SN",154,"SN",{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"54-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"126-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"138-SN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"154-SN"}]
[null,null,null,null,56,"MN",60,"MN",74,"MN",82,"MN",92,"MN",102,"MN",null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"92-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,68,"MN",82,"MN",92,"MN",102,"MN",null,null,null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"68-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"92-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,74,"MN",90,"MN",102,"MN",null,null,null,null,null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"90-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB60_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB60_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB60_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
["Table_ACB44_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[20,"TN",null,null,38,"TN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-TN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-TN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[20,"UN",null,null,38,"UN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-UN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-UN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[24,"UN",null,null,48,"UN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"48-UN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[20,"SN",null,null,64,"UN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"64-UN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[24,"SN",null,null,56,"SN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"56-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[28,"SN",null,null,64,"SN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"64-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[32,"SN",null,null,72,"SN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"32-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"72-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[36,"SN",null,null,82,"SN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"36-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"82-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[40,"SN",null,null,90,"SN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"90-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[44,"SN",null,null,98,"SN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"44-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[48,"SN",null,null,74,"MN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"48-SN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[36,"MN",null,null,82,"MN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[40,"MN",null,null,90,"MN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"90-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[44,"MN",null,null,98,"MN",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"98-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[48,"MN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"48-MN"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB44_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB44_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB44_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
[]
[]
["Table_ACB4L_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[16,"TN",26,"TN",36,"TN",46,"TN",56,"TN",68,"TN",78,"TN",88,"TN",98,"TN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"26-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"36-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"56-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"68-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"78-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"88-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"98-TN"}]
[26,"TN",34,"TN",46,"TN",56,"TN",68,"TN",82,"TN",94,"TN",106,"TN",118,"TN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"26-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"46-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"56-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"68-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"82-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"94-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"106-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"118-TN"}]
[24,"UN",42,"TN",54,"TN",66,"TN",80,"TN",98,"TN",112,"TN",126,"TN",142,"TN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"42-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"54-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"80-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"98-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"112-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"126-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"142-TN"}]
[20,"SN",36,"UN",64,"TN",78,"TN",92,"TN",114,"TN",134,"TN",148,"TN",168,"TN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"64-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"78-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"92-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"114-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"134-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"148-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"168-TN"}]
[24,"SN",42,"UN",54,"UN",66,"UN",108,"TN",96,"UN",110,"UN",124,"UN",140,"UN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"54-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"108-TN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"96-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"110-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"124-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"140-UN"}]
[20,"MN",50,"UN",60,"UN",76,"UN",90,"UN",110,"UN",126,"UN",144,"UN",162,"UN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"20-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"50-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"60-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"76-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"90-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"110-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"126-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"144-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"162-UN"}]
[22,"MN",40,"SN",70,"UN",88,"UN",104,"UN",126,"UN",144,"UN",164,"UN",186,"UN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"70-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"88-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"104-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"126-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"144-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"164-UN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"186-UN"}]
[24,"MN",44,"SN",54,"SN",68,"SN",82,"SN",98,"SN",112,"SN",128,"SN",144,"SN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"24-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"44-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"54-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"68-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"82-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"98-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"112-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"128-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"144-SN"}]
[28,"MN",48,"SN",62,"SN",78,"SN",92,"SN",110,"SN",124,"SN",144,"SN",162,"SN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"48-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"62-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"78-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"92-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"110-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"124-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"144-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"162-SN"}]
[30,"MN",36,"MN",70,"SN",88,"SN",104,"SN",124,"SN",140,"SN",162,"SN",182,"SN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"30-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"70-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"88-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"104-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"124-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"140-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"162-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"182-SN"}]
[34,"MN",40,"MN",52,"MN",66,"MN",116,"SN",138,"SN",156,"SN",180,"SN",202,"SN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"116-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"138-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"156-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"180-SN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"202-SN"}]
[36,"MN",44,"MN",58,"MN",74,"MN",86,"MN",102,"MN",114,"MN",132,"MN",150,"MN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"58-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"74-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"86-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"114-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"132-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"150-MN"}]
[null,null,48,"MN",62,"MN",82,"MN",94,"MN",112,"MN",126,"MN",146,"MN",166,"MN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"48-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"94-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"112-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"126-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"146-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"166-MN"}]
[null,null,52,"MN",68,"MN",90,"MN",106,"MN",122,"MN",138,"MN",160,"MN",180,"MN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"68-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"90-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"106-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"122-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"138-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"160-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"180-MN"}]
[null,null,56,"MN",76,"MN",98,"MN",118,"MN",134,"MN",150,"MN",174,"MN",198,"MN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"56-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"76-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"98-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"118-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"134-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"150-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"174-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"198-MN"}]
[null,null,62,"MN",82,"MN",106,"MN",132,"MN",146,"MN",164,"MN",188,"MN",214,"MN",{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"62-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"106-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"132-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"146-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"164-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"188-MN"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"214-MN"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB4L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB4L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
[]
[]
["Table_ACB5L_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[8,"SN",18,"UN",24,"UN",30,"UN",36,"UN",42,"UN",48,"UN",55,"UN",61,"UN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"8-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"18-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"24-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"48-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"55-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"61-UN"}]
[8,"MN",17,"SN",21,"SN",36,"UN",42,"UN",50,"UN",58,"UN",64,"UN",72,"UN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"8-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"17-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"21-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"50-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"58-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"64-UN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"72-UN"}]
[11,"MN",14,"MN",25,"SN",29,"SN",33,"SN",39,"SN",47,"SN",51,"SN",57,"SN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"11-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"14-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"29-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"33-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"39-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"47-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"51-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"57-SN"}]
[14,"MN",17,"MN",29,"SN",33,"SN",38,"SN",45,"SN",54,"SN",59,"SN",66,"SN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"14-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"17-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"29-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"38-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"45-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"54-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"59-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"66-SN"}]
[16,"MN",19,"MN",22,"MN",38,"SN",43,"SN",51,"SN",61,"SN",67,"SN",75,"SN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"16-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"19-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"38-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"43-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"51-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"61-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"67-SN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"75-SN"}]
[18,"MN",22,"MN",25,"MN",29,"MN",32,"MN",38,"MN",46,"MN",51,"MN",57,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"29-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"32-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"51-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"57-MN"}]
[null,null,25,"MN",28,"MN",33,"MN",36,"MN",43,"MN",52,"MN",58,"MN",65,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"33-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"36-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"43-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"58-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"65-MN"}]
[null,null,28,"MN",31,"MN",37,"MN",40,"MN",49,"MN",60,"MN",65,"MN",73,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"28-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"37-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"40-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"49-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"73-MN"}]
[null,null,31,"MN",34,"MN",41,"MN",44,"MN",54,"MN",67,"MN",73,"MN",82,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"44-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"54-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"67-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"73-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"82-MN"}]
[null,null,null,null,38,"MN",46,"MN",49,"MN",60,"MN",76,"MN",82,"MN",92,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"38-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"46-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"49-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"60-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"76-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"82-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"92-MN"}]
[null,null,null,null,41,"MN",50,"MN",54,"MN",66,"MN",84,"MN",92,"MN",102,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"41-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"50-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"54-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"66-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"84-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"92-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"102-MN"}]
[null,null,null,null,45,"MN",55,"MN",59,"MN",72,"MN",92,"MN",102,"MN",110,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"45-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"55-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"59-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"92-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"102-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"110-MN"}]
[null,null,null,null,null,null,59,"MN",65,"MN",78,"MN",99,"MN",112,"MN",119,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"59-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"78-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"99-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"112-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"119-MN"}]
[null,null,null,null,null,null,null,null,72,"MN",85,"MN",null,null,null,null,126,"MN",{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"85-MN"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"126-MN"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB5L_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB5L_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[]
[]
[]
[]
[]
[]
["Table_ACB25_Nozzle_4"]
["2_Count","2_Nozzle","3_Count","3_Nozzle","4_Count","4_Nozzle","5_Count","5_Nozzle","6_Count","6_Nozzle","7_Count","7_Nozzle","8_Count","8_Nozzle","9_Count","9_Nozzle","10_Count","10_Nozzle","2_C","3_C","4_C","5_C","6_C","7_C","8_C","9_C","10_C"]
[17,"TN",null,null,34,"TN",null,null,51,"TN",null,null,67,"TN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"17-TN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"34-TN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"51-TN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"67-TN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[18,"UN",null,null,30,"UN",null,null,61,"TN",null,null,81,"TN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"18-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"30-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"61-TN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"81-TN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[17,"SN",null,null,36,"UN",null,null,52,"UN",null,null,69,"UN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"17-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"36-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"52-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"69-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[21,"SN",null,null,42,"UN",null,null,61,"UN",null,null,81,"UN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"21-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"61-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"81-UN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[17,"MN",null,null,33,"SN",null,null,48,"SN",null,null,64,"SN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"17-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"33-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"48-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"64-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[19,"MN",null,null,37,"SN",null,null,55,"SN",null,null,74,"SN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"19-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"37-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"55-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"74-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[22,"MN",null,null,42,"SN",null,null,63,"SN",null,null,84,"SN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"22-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"42-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"63-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"84-SN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[25,"MN",null,null,31,"MN",null,null,47,"MN",null,null,63,"MN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"25-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"31-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"47-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"63-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,35,"MN",null,null,53,"MN",null,null,71,"MN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"35-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"53-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"71-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,39,"MN",null,null,59,"MN",null,null,79,"MN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"39-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"59-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"79-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,43,"MN",null,null,65,"MN",null,null,87,"MN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"43-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"65-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"87-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,47,"MN",null,null,72,"MN",null,null,96,"MN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"47-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"72-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"96-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,52,"MN",null,null,79,"MN",null,null,106,"MN",null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"52-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"79-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"106-MN"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_ACB25_Nozzle_4[[#This Row],[2_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[2_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[3_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[3_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[4_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[4_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[5_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[5_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[6_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[6_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[7_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[7_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[8_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[8_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[9_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[9_Nozzle]]","v":"-"},{"$f":"Table_ACB25_Nozzle_4[[#This Row],[10_Count]]&\"-\"&Table_ACB25_Nozzle_4[[#This Row],[10_Nozzle]]","v":"-"}]

{"sheet":"ACB Format Handler","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Data Validation","index":6,"n_rows":92,"n_cols":59,"rows_kept":92,"cut":false,"hidden":true,"merged":[[0,56,0,58],[5,8,6,8],[5,20,6,20],[0,50,0,54],[1,31,1,47],[10,12,11,12],[10,14,11,14],[6,11,6,12],[10,10,11,10],[10,11,11,11],[10,13,11,13],[5,14,6,14],[18,9,18,11],[18,4,18,8],[13,1,13,2],[13,3,13,6],[12,11,12,12],[18,12,18,36],[10,1,10,2],[10,3,10,6],[10,9,11,9],[14,1,14,2],[14,3,14,6],[10,8,12,8],[12,1,12,2],[12,3,12,6],[11,1,11,2],[11,3,11,6],[16,37,16,47],[17,37,17,41],[17,42,17,45],[17,46,17,47],[18,39,18,40],[18,37,18,38],[18,44,18,45],[18,42,18,43]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Spigot Shapes",null,null,null,null,null,"Spigot Sizes"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grilles"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB40_G","ACB50_G","FMVBY_G","FMLBY_G","FMTBY_G","ACB10_G","ACB20_G","ACB30_G","ACB35_G","ACB45_G","ACB55_G","ACB3L_G","ACB60_G","ACB44_G","ACB4L_G","ACB5L_G","ACB25_G",null,null,"ACB40",null,null,null,null,null,"ACB40",null,"ACB50"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8","10"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","N/A","N/A","N/A","Unattached Bar Grille","N/A","Vertical Throw","Vertical Throw","N/A","N/A","Vertical Throw","Exposed","N/A","N/A","N/A","N/A",null,null,null,null,null,null,null,null,4,null,4]
[null,null,null,null,null,null,null,null,"Room Conditions","Dry Bulb","Relative Humidity","Dew Point","On-Coil Air Temp",null,"Primary Air Conditions","Dry Bulb","Relative Humidity","Wet Bulb","Dew Point",null,"Enter Water Temp","Entering Water","Propylene Glycol","Ethylene Gylcol",null,"Elevation",null,null,null,null,null,null,null,null,null,null,"Attached Bar Grille",null,"1-Way LVD","1-Way LVD",null,null,"1-Way LVD","Flush Mounted",null,null,null,null,null,null,"Round","Round","Round","Elliptical","Round",null,5,null,5]
[null,null,null,null,null,null,null,null,null,"°F","%","°F",null,null,null,"°F","%","°F",null,null,null,"°F","%","%",null,"ft",null,null,null,null,null,null,null,null,null,null,null,null,"2-Way LVD","2-Way LVD",null,null,"2-Way LVD",null,null,null,null,null,null,null,null,null,null,"Round",null,null,6,null,6]
[null,null,null,null,null,null,null,null,"Min",40,0,null,40,null,"Min",40,0,null,null,null,"Min",40,0,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,8]
[null,null,null,null,null,null,null,null,"Max",120,100,null,120,null,"Max",120,100,null,null,null,"Max",200,20,20,null,30000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB50",null,null,null,null,null,10,null,10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8","10"]
[null,"Project Name:",null,null,null,null,null,null,"Global Constraints","Air ∆P","H2O ∆P","Cooling","Heating","Sound Level","Primary Air / Linear Ft.",null,null,null,null,null,null,null,30,30]
[null,"Project Number:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Elliptical","Round",null,"ACB20",null,"ACB4L"]
[null,"Version:",null,null,null,null,null,null,null,"Inch WC","ft WC","GPM",null,"NC","CFM / Lft",null,null,null,null,null,null,null,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round"]
[null,"Date:",null,null,null,null,null,null,"Min",0.1,0.1,0.2,0.2,0,3,null,null,null,null,null,null,null,45,45,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,4]
[null,"Software Version:",null,null,null,null,null,null,"Max",3,22,2.4,2.4,50,50,null,null,null,null,null,null,null,50,50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB20",null,null,null,null,null,5,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8","10",null,6,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Local Design Conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Room Conditions",null,null,null,null,"Primary Air Conditions",null,null,null,"Entering Water",null,null,null,"Round","Round","Round","Elliptical","Round",null,10]
[null,null,null,null,"Design Requirements",null,null,null,null,"Load Difference",null,null,"Design Criteria",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling",null,"Heating",null,"Cooling","Cooling",null,"Heating",null,"Cooling","Heating",null,null,null,null,null,"Round"]
[null,"Unit Tag","Zone Name or Number","Area","Sensible Load","Latent Load","Heating Load","Min. Outside Air or Primary Airflow","Number of Units","Sensible","Latent","Heating","Model","Model Length_ACB40","Model Length_ACB50","Model Length_FMVBY","Model Length_FMLBY","Model Length_FMTBY","Model Length_ACB10","Model Length_ACB20","Model Length_ACB30","Model Length_ACB35","Model Length_ACB45","Model Length_ACB55","Model Length_ACB3L","Model Length_ACB60","Model Length_ACB44","Model Length_ACB4L","Model Length_ACB5L","Model Length_ACB25","Model Length_","Model Length_Select Unit","Chilled Water Flow Rate","Water Pressure Drop (Cooling)","Heating Water Flow Rate","Water Pressure Drop (Heating)","Sound Level","Dry Bulb","Relative Humidity","Dry Bulb2","Relative Humidity2","On-Coil Air Temp","Dry Bulb3","Relative Humidity3","Dry Bulb4","Relative Humidity4","Entering Water","Entering Water2",null,null,null,null,null,null,null,null,null,null,"ACB60"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,0,40,0,40,40,0,40,0,40,40,null,null,"ACB4L",null,null,null,null,null,"ACB5L"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB40",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,null,null,null,null,null,120,100,120,100,120,120,100,120,100,200,200,null,null,"4","5","8","10",null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB50",4,4,3,3,3,3,4,3,3,4,4,3,4,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB45",6,6,4,4,4,4,6,4,4,6,6,4,6,null,6,6,6,6,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Oval","Oval",null,null,5,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB55",8,8,5,5,5,5,8,5,5,8,8,5,8,null,8,8,8,8,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB60",10,10,6,6,6,6,10,6,6,10,10,6,10,null,10,10,null,10,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB30",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB5L"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB35",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","8","10"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB4L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FMTBY",null,"FMLBY"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB5L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Oval","Oval"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB10",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB20"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ACB44",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB60"]
[null,null,null,null,null,null,null,null,null,null,null,null,"FMLBY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8",null,null,"FMVBY",null,"ACB30"]
[null,null,null,null,null,null,null,null,null,null,null,null,"FMTBY"]
[null,null,null,null,null,null,null,null,null,null,null,null,"FMVBY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Elliptical",null,null,4,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FMTBY",null,"FMVBY",null,"FMLBY",null,"ACB3L",null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4",null,"4",null,"4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round",null,"Round",null,"Round",null,5,null,"ACB35"]
[null,"ACB40",null,null,null,null,null,null,null,null,null,null,"ACB60",null,null,null,null,null,null,null,null,null,null,"ACB4L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,4]
[null,2,2,2,2,2,2,2,2,2,2,null,2,2,2,2,2,2,2,2,2,2,null,2,2,2,2,2,2,2,2,2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB30",null,null,null,null,null,null,null,5]
[null,4,4,4,4,4,4,4,4,4,4,null,4,4,4,4,4,4,4,4,4,4,null,4,4,4,4,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8",null,null,null,null,6]
[null,null,null,null,null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,null,null,null,null,null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,null,null,null,null,null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB10",null,8]
[null,null,null,null,null,"4 - DC","4 - DC","4 - DC","4 - DC","4 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 - DC","4 - DC","4 - DC","4 - DC","4 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Round"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,"ACB45"]
[null,"ACB50",null,null,null,null,null,null,null,null,null,null,"ACB30",null,null,null,null,null,null,"ACB3L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB3L",null,null,null,null,null,6]
[null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,"2_L","3_L","4_L","5_L","6_L","_L",null,"2_L","3_L","4_L","5_L","6_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8",null,null,8,null,4]
[null,2,2,2,2,2,2,2,2,2,2,null,2,2,2,2,2,2,null,2,2,2,2,2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
[null,4,4,4,4,4,4,4,4,4,4,null,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oval","Round","Oval","Oval",null,null,null,null,6]
[null,null,null,null,null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,null,null,null,null,null,"2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round",null,null,null,null,null,"ACB55",null,8]
[null,null,null,null,null,"4 - DC","4 - DC","4 - DC","4 - DC","4 - DC",null,null,null,null,null,null,null,null,null,"ACB10"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2_L","3_L","4_L","5_L","6_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB35",null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2,2,2,2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8",null,null,5]
[null,"ACB45",null,null,null,null,null,null,null,null,null,null,"ACB35",null,null,null,null,null,null,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,"2_L","3_L","4_L","5_L","6_L","_L",null,null,null,null,null,"2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Oval",null,null,8,null,"Blank"]
[null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,2,2,2,2,2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oval"]
[null,4,4,4,4,4,4,4,4,4,4,null,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB10",null,null,null,null,null,"ACB44"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB20",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8"]
[null,"ACB55",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","10_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,"ACB25"]
[null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,null,null,null,null,null,null,null,2,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Oval",null,null,5]
[null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",2,null,"FMLBY",null,null,null,null,null,null,4,"4 - DC","4 - DC","4 - DC","4 - DC","4 - DC","4 - DC","4 - DC","4 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oval","Elliptical",null,null,6,null,4]
[null,4,4,4,4,4,4,4,4,4,4,null,"2_L","3_L","4_L","5_L","6_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,2,2,2,2,2,2,null,"FMTBY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB45",null,null,null,null,null,10,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,4,4,4,4,4,4,null,"2_L","3_L","4_L","5_L","6_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8",null,null,null,null,8]
[null,"FMVBY",null,null,null,null,null,null,"ACB44",null,null,null,null,null,null,null,"2 - DC",null,null,2,2,2,2,2,2]
[null,"2_L","3_L","4_L","5_L","6_L","_L",null,"2_L","4_L","_L",null,null,null,null,null,null,null,null,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Elliptical"]
[null,2,2,2,2,2,2,null,2,"2 - DC",2,null,null,null,null,null,null,null,null,null,null,null,null,"2 - DC"]
[null,4,4,4,4,4,4,null,4,"4 - DC",4]
[null,null,null,null,null,"2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB55"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Elliptical"]
[null,"ACB5L",null,null,null,null,null,null,null,null,null,null,"Blank"]
[null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L"]
[null,2,2,2,2,2,2,2,2,2,2,null,2,2,2,2,2,2,2,2,2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Blank",null,"ACB25"]
[null,4,4,4,4,4,4,4,4,4,4,null,4,4,4,4,4,4,4,4,4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4",null,"4","5","6","8"]
[null,null,null,null,null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC",null,null,null,null,null,null,"2 - DC","2 - DC","2 - DC","2 - DC","2 - DC"]
[null,null,null,null,null,"4 - DC","4 - DC","4 - DC","4 - DC","4 - DC",null,null,null,null,null,null,"4 - DC","4 - DC","4 - DC","4 - DC","4 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round",null,"Round","Round","Round","Round"]
[]
[]
[null,"ACB25",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACB44"]
[null,"2_L","3_L","4_L","5_L","6_L","7_L","8_L","9_L","10_L","_L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4","5","6","8","10"]
[null,2,null,2,null,2,null,2,null,null,2]
[null,4,null,4,null,4,null,4,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round","Round","Round","Elliptical","Round"]
[null,null,null,null,null,"2 - DC",null,"2 - DC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round"]
[null,null,null,null,null,"4 - DC",null,"4 - DC"]

{"sheet":"Username Archive","index":7,"n_rows":2,"n_cols":7,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["wfhq_coski","2019-04-03",null,"Unit","Coil","Length","Count"]
["wfhq_slamica","2019-04-03"]

{"sheet":"Changelog","index":8,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Date","Version","Changes"]
["2019-04-02",1.01,"software released"]